**Date: 25/11/2014**

**Amendment No: 1**

**Ref: Tender Enquiry No: HLL/BME/Calibration-04/14-15 Dated 18.11.2014**

Pre-Bid meeting against the referred tender was held on **25/11/2014** at HLL Lifecare Ltd., Thycaud, Trivandrum- 695 014

The following amendments are issued with respect to the above Tender Enquiry Document.

**Technical Specification**

**Item No. 4**

|  |  |
| --- | --- |
| **S.N** | **Semi Micro Balance for Pipette Calibration** |
| **1** | **Operationg Requirement** |
| 1.1 | Precision semi microbalance system with pipette calibration kit |
| **2** | **Technical Specification** |
| 2.1 | It should have high resolution 5" graphical display |
| 2.2 | It should have automatic motorized leveling |
| 2.3 | Should be supplied with a an automatic draft shield |
| 2.4 | Readability: 0.01mg |
| 2.5 | Max capacity: 220g |
| 2.6 | Repeatability: 0.02mg |
| 2.7 | Should have USB interface for connecting to PC |
| 2.8 | Should be supplied with all necessary pipette calibration kit/set |
| 2.9 | Should have pipette calibration software (Optional) |
| 2.10 | Should supply with E2 calibration weights |
| **3** | **Standards, Safety and Calibration** |
| 3.1 | Comprehensive warranty for 2 years |
| 3.2 | During the warranty period, the equipment should be calibrated free of cost |
| 3.3 | Equipment should be European CE/US FDA approved. |
| 3.4 | Comprehensive training for HLL staff till familiar with the system. |
| 3.5 | Manufacturer should have valid ISO 13485 certification (copy should be attached with the quote) |
| 3.6 | Should be supplied with valid calibration certificate |
| 3.7 | Should be supplied with user Manual (English), Service manual/calibration manual (English) |

***Amended as:***

|  |  |
| --- | --- |
| **S.N** | **Semi Micro Balance for Pipette Calibration** |
| **1** | **Operation Requirement** |
| 1.1 | Precision semi microbalance system with pipette calibration kit |
| **2** | **Technical Specification** |
| 2.1 | ***It should have high resolution 5” display.*** |
| 2.2 | ***It should have automatic leveling.*** |
| 2.3 | ***Should have provision for draft shield.*** |
| 2.4 | Readability: 0.01mg |
| 2.5 | Max capacity: 220g |
| 2.6 | Repeatability: 0.02mg |
| 2.7 | Should have USB interface for connecting to PC |
| 2.8 | Should be supplied with all necessary pipette calibration kit/set |
| 2.9 | Should have pipette calibration software (Optional) |
| 2.10 | Should supply with E2 calibration weights |
| **3** | **Standards,Safety and Calibration** |
| 3.1 | Comprehensive warranty for 2 years |
| 3.2 | During the warranty period, the equipment should be calibrated free of cost |
| 3.3 | Equipment should be European CE/US FDA approved. |
| 3.4 | Comprehensive training for HLL staff till familiar with the system. |
| 3.5 | Manufacturer should have valid ISO 13485 certification (copy should be attached with the quote) |
| 3.6 | Should be supplied with valid calibration certificate |
| 3.7 | Should be supplied with user Manual (English), Service manual/calibration manual (English) |

**All other contents, terms & conditions of the tender enquiry remain unchanged.**