|  |  |  |
| --- | --- | --- |
|  | **Tendered Specification** | **Amendments** |
| 1 | “Fully automatic oxygen control panel –Imported “mentioned in Para 1.2 of technical specification. | Fully automatic oxygen control panel –Imported wih CE certification. |
| 2 | “Duplex Anesthetic Gas Scavenging System (AGSS) of 500 l/min -Imported “mentioned in Para 4 of technical specification. | Duplex Anesthetic Gas Scavenging System (AGSS) of 500 l/min –Imported with CE certification |
| 3 | “Operating theatres shall be equipped with single arm moveable pendants suspended from the ceiling “mentioned in Para 14 of technical specification. | Operating theatres shall be equipped with rigid pendants suspended from the ceiling |
| 4 | “Oxygen Flow meter with Humidifier Bottle and probe key- Supply installation, testing and commissioning of anodized aluminum oxygen flow meter with humidifier bottle 0-10Litres. **–Indigenous”**  mentioned in Para 11 of detailed BOQ | Oxygen Flow meter with Humidifier Bottle and probe key- Supply installation, testing and commissioning of oxygen flow meter with humidifier bottle 0-10Litres. **–Indigenous** |
| 5 | “Semi-Automatic Nitrogen Control System : Supply, Installation testing and commissioning of Fully Automatic Nitrogen Control System-**Indigenous”** mentioned in Para 13 of detailed BOQ | “Semi-Automatic Nitrous oxide Control System : Supply, Installation testing and commissioning of semi Automatic Nitrous oxide Control System-**Indigenous”** |

**Minutes of the prebid meeting for the Supply Installation, Testing and Commissioning of Medical gas pipe line system at the first floor of TH Karunagapally.**

The quoted rate should be inclusive of all applicable taxes including the **work contract tax.**

There should be two years warranty for the entire MGPS system excluding oxygen flowmeter and ward vacuum unit.