|  |  |  |
| --- | --- | --- |
| Sl No | Original as per tender | Amended Specification |
| 1 | **Torch- Local Purchase** | |  | | --- | | LED type torch | | Should be supplied with rechargeable batteries and charger | | Should be suitable for clinical application | |
| 2 | **Vacuum Cleaner- Local Purchase** | |  | | --- | | Should have minimum 1200 Watts of Powerful Suction | | Blower efficiency 30-35lt/sec | | Should be suitable for wet and dry application | | Power supply: 230V,50 Hz | |
| 3 | **Oxygen Cylinder With Gauge- Local Purchase** | |  | | --- | | Should be type B oxygen cylinder with regulator and gauge | | Should be with oxygen flow meter with humidifier bottle attached to the regulator | | Should be supplied with portable oxygen trolley made up of MS | |
| 4 | **Cidex Tray- Local Purchase** | |  | | --- | | Should be made up of polypropylene | | Heat resistant up to 134 degree Celsius | | Approximate Dimension : 750 mm X 220 mm X 130mm ( 14 litres) | | Should be supplied with lid | |
| 5 | **Emergency Lamp- Local Purchase** | |  | | --- | | Should be rechargeable emergency light | | Brightness should be 1000 lumens or more | | Should provide minimum 4 hours back up | | Should be LED based or CFL based | | Should be supplied with all accessories | |